Table 5. Orthogonal test factors at each level.
	Level
	Voltage
	Electrode spacing
	Electrode arrangement
	Moisture content
	Degree of vacuum 

	1
	15 V
	10 cm
	Double row
	30%
	0.05–0.06 MPa

	2
	20 V
	15 cm
	Quadrilateral
	42%
	

	3
	25 V
	20 cm
	Hexagon
	54%
	



