Table: 1
	Model
	kp
	ki
	kd
	Overshoot %
	Settling Time in Second

	Conventional PID Controller
	2.01
	0.18
	1.65
	18.68
	1.8

	LSTM Based Controller
	2.35
	0.11
	3.20
	0.45
	0.6
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