{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Experimental data"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Experimental data","index":0,"n_rows":392,"n_cols":6,"rows_kept":392,"merged":[[2,5,2,9],[80,1,80,4]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
["Figure 2: Variation of Brake Thermal Efficiency at different load condition"]
[]
["LOAD  ( % )","DIESEL","32 DEG C","50 DEG C","15% EGR"]
[0]
[20,14.51,7.8,8.6,8.6]
[40,23.35,13.3,14.2,14.4]
[60,28.71,18,19.3,18.6]
[80,30.97,21.8,23.4,21.1]
[100,31.35,24.1,25.8,22.7]
[]
[]
[]
["Figure3: Variation of Hydrocarbon emission versus various loads"]
[]
["LOAD  ( % )","DIESEL","32 DEG C","50 DEG C","15% EGR"]
[0,30,2250,2010,1950]
[20,45,1950,1650,1770]
[40,80,1500,1290,1395]
[60,105,1010,795,980]
[80,128,870,675,1010]
[100,139,710,520,1030]
[]
[]
[null,"C0  EMISSIONS"]
["Figure 4: Variation of Carbon Monoxide versus loads "]
[]
["LOAD  ( % )","DIESEL","32 DEG C","50 DEG C",{"v":0.15,"d":"15%"}]
[0,0.08,0.59,0.54,0.55]
[20,0.09,0.51,0.46,0.45]
[40,0.1,0.43,0.35,0.43]
[60,0.12,0.34,0.29,0.39]
[80,0.15,0.27,0.23,0.4]
[100,0.19,0.21,0.17,0.41]
[]
[]
[]
["Figure 5: Variation of of Nitric Oxide at various load condition"]
[]
["LOAD  ( % )","Diesel","32 DEG C","50 DEG C",{"v":0.15,"d":"15%"}]
[0,110,40,77,17]
[20,250,70,120,40]
[40,420,115,165,45]
[60,705,170,229,75]
[80,975,348,433,160]
[100,1220,425,550,205]
[]
[]
["Figure 6: Relationships between Smoke level and various loads"]
[]
["LOAD  ( % )","Diesel","32 DEG C","50 DEG C",{"v":0.15,"d":"15%"}]
[0]
[20,0.6,0.1,0.03,0.3]
[40,1.1,0.2,0.1,0.5]
[60,1.5,0.3,0.15,0.7]
[80,2.6,0.5,0.2,1.4]
[100,3.8,0.6,0.25,1.6]
[]
[]
[]
["Figure 7: Results of exhaust gas temperature for various loads"]
[]
[null,"EXHASUT GAS TEMPERATURE"]
[]
[null,"LOAD  ( % )","Diesel","32 DEG C","50 DEG C",{"v":0.15,"d":"15%"}]
[null,0,170,180,202,142]
[null,20,195,210,235,175]
[null,40,265,235,263,185]
[null,60,335,285,333,235]
[null,80,425,370,425,300]
[null,100,530,475,520,410]
[]
[]
[]
[]
["Figure 8: Results of peak pressure for various loads"]
[]
[]
[null,"LOAD %","DIESEL","LPG","50 DEG C",{"v":0.15,"d":"15%"}]
[null,0,49.65,33.4,34.2,34.24]
[null,20,54.55,34.54,35.64,35.64]
[null,40,59.54,37.48,38.78,37.9]
[null,60,62.75,42.59,44.2,41.74]
[null,80,66.1,48.12,50.22,46.92]
[null,100,67.56,51.8,55,50]
[]
[]
[]
[]
[]
["Figure 9:   Experimental result of pressure crank – angle diagram at full load"]
[]
["Crank Angle","Diesel","LPG","EGR","600 C hot Air"]
[300,0,0.500977517106549,0.249266862170088,0.935972629521017]
[301,0,0.532746823069404,0.351906158357771,1.06549364613881]
[302,0,0.564516129032258,0.503421309872923,1.20478983382209]
[303,0,0.598729227761486,0.703812316715542,1.41251221896383]
[304,0,0.650048875855328,0.972629521016618,1.57624633431085]
[305,0,0.701368523949169,1.2316715542522,1.80351906158358]
[306,0,0.689149560117302,1.45650048875855,2.00879765395894]
[307,0.00391006842619746,0.799120234604106,1.68132942326491,2.29472140762463]
[308,0.0156402737047898,0.857771260997067,1.95992179863148,2.58064516129032]
[309,0.0234604105571848,0.935972629521017,2.24095796676442,2.89100684261975]
[310,0.072336265884653,1.06549364613881,2.52932551319648,3.25513196480938]
[311,0.127077223851417,1.20478983382209,2.88856304985337,3.59481915933529]
[312,0.252199413489736,1.41251221896383,3.24535679374389,4.03714565004888]
[313,0.447702834799609,1.57624633431085,3.59237536656891,4.49902248289345]
[314,0.547409579667644,1.80351906158358,4.02737047898338,4.83870967741936]
[315,0.914956011730205,2.00879765395894,4.29863147605083,5.38367546432063]
[316,1.12218963831867,2.29472140762463,4.78005865102639,5.9822]
[317,1.43890518084066,2.58064516129032,5.20039100684262,6.2544]
[318,1.78885630498534,2.89100684261975,5.66715542521994,7.26665]
[319,1.97849462365591,3.25513196480938,6.16813294232649,7.354]
[320,2.38318670576735,3.59481915933529,6.6911045943304,7.8954]
[321,2.6158357771261,4.03714565004888,7.13587487781036,9.25478]
[322,3.01270772238514,4.49902248289345,7.79814271749756,10.235487]
[323,3.54838709677419,4.83870967741936,8.39442815249267,11.2354]
[324,3.79667644183773,5.38367546432063,9.02737047898338,12.2354]
[325,4.32844574780059,5.87243401759531,9.66764418377322,13.2565]
[326,4.82111436950147,6.341642228739,10.3690127077224,14.23654]
[327,5.2297165200391,6.90615835777126,11.0459433040078,15.1454]
[328,5.83773216031281,7.52199413489736,11.8572825024438,16.15247]
[329,6.1485826001955,8.11827956989247,12.6099706744868,17.02457]
[330,6.81915933528837,8.70723362658847,13.4384164222874,18.0245]
[331,7.48582600195503,9.45503421309873,14.286412512219,19.032145]
[332,8.01759530791789,10.1026392961877,15.1075268817204,20.12457]
[333,8.81524926686217,10.8528836754643,15.9897360703812,21.02154]
[334,9.21603128054741,11.6495601173021,16.9916911045943,22.0154]
[335,10.1329423264907,12.4462365591398,17.8445747800587,23.01547]
[336,10.9657869012708,13.3773216031281,18.9345063538612,24.23558]
[337,11.5855327468231,14.1764418377322,19.8020527859238,25.6325]
[338,12.6588465298143,15.1612903225806,20.9701857282502,26.7124]
[339,13.2023460410557,16.1168132942326,22.0307917888563,27.8154]
[340,14.3108504398827,17.0967741935484,23.108504398827,28.9214]
[341,15.2570869990225,18.2184750733138,24.3352883675464,29.541]
[342,16.0723362658847,19.2155425219941,25.183284457478,30.6547]
[343,17.3352883675464,20.3714565004888,26.3782991202346,31.7854]
[344,18.0254154447703,21.4051808406647,27.3289345063539,32.89547]
[345,19.286412512219,22.5733137829912,28.1964809384164,34.2578]
[346,20.6080156402737,23.7487781036168,29.2350928641251,34.89578]
[347,21.247311827957,24.9291300097752,30.563254,36.21547]
[348,22.5826001955034,26.2487781036168,31.9632547,40.254]
[349,23.1827956989247,27.3387096774194,33.523254,42.254]
[350,24.4144672531769,28.7145650048876,34.756258,42.9687]
[351,25.5581622678397,29.7873900293255,35.963254,44.23547]
[352,26.1329423264907,31.0581622678397,37.162547,46.32547]
[353,27.2961876832845,32.2605083088954,38.4852147,47.9654]
[354,27.8885630498534,33.330889540567,40.8632547,49.326587]
[355,30.0351906158358,35.2443792766373,41.5632587,51.0231457]
[356,36.9364613880743,36.9281524926686,43.5230214,52.36587]
[357,40.5024437927664,38.8685239491691,44.532147,53.26658]
[358,45.9511241446725,40.3885630498534,45.8632547,54.32564]
[359,49.0185728250244,42.36598,46.35978935,54.98778]
[360,54.4086021505376,43.8660801564027,47.0101324,55]
[361,59.2434017595308,45.125487,47.3213354,54.986741]
[362,61.266862170088,47.123698,47.0230214,54]
[363,64.8132942326491,48.9632547,46.32776805,53]
[364,66.0684261974585,50.6325478,45.6325147,51]
[365,67.5620723362659,51.236587,44.4325471,49]
[366,67.5034213098729,51.802154,42.9692082111437,47]
[367,66.9188660801564,51.564239735,42.0821114369501,45]
[368,64.9560117302053,51.32632547,40.9457478005865,43]
[369,63.7399804496579,50.2362547,39.6700879765396,41]
[370,61.5483870967742,48.799401700000004,38.6999022482893,39]
[371,59.6148582600196,47.3625487,37.4437927663734,36]
[372,58.7057673509286,45.3201457,36.1510263929619,33]
[373,57.1749755620723,42.6759530791789,34.7482893450635,31]
[374,56.3929618768328,41.04227761485825,33.3357771260997,29]
[375,54.6275659824047,39.4086021505376,31.766862170088,27]
[376,52.6001955034213,37.9667644183773,30.3983382209189,26]
[377,51.4486803519062,36.5933528836755,28.9100684261975,25]
[378,49.0420332355816,35.3152492668622,27.6710654936461,24]
[379,47.3352883675464,33.8391984359726,26.4565004887586,23]
[380,45.2434017595308,33.2632547,25.1539589442815,22]
[381,42.8387096774194,31.73915423172045,23.9931573802542,21]
[382,41.6304985337243,30.2150537634409,22.9130009775171,20]
[383,39.3509286412512,28.5386119257087,21.8401759530792,19.7]
[384,37.9491691104594,27.63254174,20.9090909090909,19.1]
[385,36.1348973607038,26.264014369999998,19.9022482893451,18.4]
[386,34.0899315738025,24.895487,19.0420332355816,17.5]
[387,33.1143695014663,23.12548,18.1329423264907,16.5]
[388,31.2258064516129,22.00012,17.2629521016618,16]
[389,30.0293255131965,21.12547,16.5127077223851,15.8]
[390,28.5219941348974,20.274518999999998,15.6500488758553,15.1]
[391,26.8035190615836,19.423568,14.9853372434018,14.5]
[392,25.9706744868035,18.236985,14.2424242424242,13.8]
[393,24.3010752688172,17.4678695,13.5434995112414,12.8]
[394,23.3685239491691,16.698754,12.9081133919844,12.4]
[395,22.1036168132942,16.132658,12.2238514173998,11.9]
[396,20.7370478983382,15.549069,11.6544477028348,10.8]
[397,20.0547409579668,14.96548,11.0728250244379,10.4]
[398,18.772238514174,14.15487,10.5547409579668,10]
[399,17.5581622678397,13.475073313783,10.000121,9.5]
[400,17.0087976539589,12.925219941349,9.52101661779081,9]
[401,15.8240469208211,12.3435972629521,9.01270772238514,8.7]
[402,15.2707722385142,11.536987,8.56549364613881,8]
[403,14.2561094819159,11.003214,8.09628543499511,7.52443792766373]
[404,13.3567937438905,10.326598,7.66862170087976,7.23607038123167]
[405,12.9169110459433,9.950689029325515,7.31671554252199,7.06500488758553]
[406,12.0175953079179,9.57478005865103,6.90615835777126,6.74975562072336]
[407,11.6383186705767,9.36461388074291,6.59335288367546,6.50293255131965]
[408,10.7663734115347,8.92717497556207,6.21212121212121,6.20478983382209]
[409,10.0742913000978,8.73900293255132,5.94086021505376,5.91397849462366]
[410,9.71456500488759,8.3455522971652,5.58406647116325,5.68426197458456]
[411,8.94037145650049,7.95698924731183,5.30058651026393,5.42766373411535]
[412,8.70576735092864,7.52443792766373,5.01221896383187,5.32154]
[413,8.05083088954057,7.23607038123167,4.73118279569893,4.91236]
[414,7.43695014662757,7.06500488758553,4.48435972629521,4.54879]
[415,7.20821114369501,6.74975562072336,4.22287390029326,4.17897]
[416,6.65102639296188,6.50293255131965,4.02248289345064,4.021547]
[417,6.33040078201369,6.20478983382209,3.75610948191593,3.803295]
[418,5.92766373411535,5.91397849462366,3.57771260997067,3.58504398826979]
[419,5.41544477028348,5.68426197458456,3.33333333333333,3.33822091886608]
[420,5.20039100684262,5.42766373411535,3.14516129032258,3.10117302052786]
[421,4.65298142717498,5.32154,2.94721407624633,2.9227761485826]
[422,4.48484848484849,4.91236,2.70772238514174,2.72727272727273]
[423,4.1564027370479,4.54879,2.56109481915934,2.60752688172043]
[424,3.76344086021505,4.17897,2.38514173998045,2.39980449657869]
[425,3.57966764418377,4.021547,2.21896383186706,2.25317693059629]
[426,3.22189638318671,3.803295,2.03323558162268,2.03567937438905]
[427,3.01661779081134,3.58504398826979,1.89882697947214,1.93792766373412]
[428,2.73900293255132,3.33822091886608,1.79863147605083,1.82795698924731]
[429,2.43206256109482,3.10117302052786,1.61534701857283,1.70821114369501]
[430,2.3030303030303,2.9227761485826,1.4980449657869,1.54936461388074]
[431,2.0019550342131,2.72727272727273,1.34408602150538,1.44428152492669]
[432,1.81427174975562,2.60752688172043,1.23900293255132,1.3782991202346]
[433,1.59726295210166,2.39980449657869,1.09726295210166,1.24389051808407]
[434,1.36070381231672,2.25317693059629,0.997067448680352,1.1485826001955]
[435,1.22189638318671,2.03567937438905,0.894428152492669,1.04349951124145]
[436,0.975562072336266,1.93792766373412,0.784457478005865,0.967741935483871]
[437,0.844574780058651,1.82795698924731,0.71603128054741,0.909090909090909]
[438,0.666666666666667,1.70821114369501,0.571847507331378,0.83088954056696]
[439,0.475073313782991,1.54936461388074,0.500977517106549,0.772238514173998]
[440,0.404692082111437,1.44428152492669,0.447214076246334,0.713587487781036]
[441,0.27761485826002,1.3782991202346,0.366568914956012,0.679374389051808]
[442,0.207233626588465,1.24389051808407,0.298142717497556,0.554740957966764]
[443,0.134897360703812,1.1485826001955,0.217497556207234,0.537634408602151]
[444,0.0801564027370479,1.04349951124145,0.161290322580645,0.513196480938416]
[445,0.0488758553274682,0.967741935483871,0.136852394916911,0.412569]
[446,0.021505376344086,0.909090909090909,0.095307917888563,0.369874]
[447,0.0136852394916911,0.83088954056696,{"v":0.0806451612903226,"d":"8.06E-02"},0.298574]
[448,0.00782013685239492,0.772238514173998,{"v":0.0562072336265885,"d":"5.62E-02"},0]
[449,0.00195503421309873,0.713587487781036,{"v":0.0439882697947214,"d":"4.40E-02"},0]
[450,0,0.679374389051808,{"v":0.0293255131964809,"d":"2.93E-02"}]
[451,0,0.554740957966764]
[452,0,0.537634408602151]
[453,0,0.513196480938416]
[454,0,0.412569]
[455,0,0.369874]
[456,0,0.298574]
[457,0,0]
[458,0,0]
[459,0]
[460,0]
[]
[]
[]
["Figure 10: Experimental result of heat release rate at full load"]
[]
["Crank","Diesel","LPG Base","15 %EGR","60 Deg"]
[330,0,-0.5,-0.5,-0.5]
[331,-1,-0.9,-0.9,-0.6]
[332,-1.05,-0.6,-0.6,-0.9]
[333,-1.02,-1,0.2,-0.99]
[334,-1.05,-0.7,0.7,0.1]
[335,-1.01,0.4,0.5,0.89]
[336,-2.02,0.8,0.7,0.12]
[337,-1.06,0.3,1.1,0.35]
[338,-2.05,1.01,0.8,0.5]
[339,-2.01,0.2,1.1,0.35]
[340,-0.863214,0.3,0.4,0.47]
[341,0.0232147,0.6,0.8,0.89]
[342,-0.98632,0.8,0.3,2.4]
[343,0.236214,1,1.01,3.8]
[344,-0.89632,2.9,0.2,1.9]
[345,-0.15214,5,0.5,1]
[346,1.230147,2.5,0.2,0.68]
[347,1.0214,1.4,1.2,0.12]
[348,1.652014,0.5,2.9,0.5]
[349,0,0.6,5.8,0.32]
[350,1.963214,0.8,3,1.5]
[351,0,0.3,1.3,1]
[352,5,1.2,0.8,4.1]
[353,10,0.5,0.2,12]
[354,50,1.1,0.1,22]
[355,92,0.8,1,34]
[356,68,3,0.3,49]
[357,40,12,1.4,63]
[358,19,20,2.5,69]
[359,14,35,6.8,62]
[360,24,52,14,48]
[361,21.5,62,23,38]
[362,17,59,36,25]
[363,20,50,47,15]
[363.5,21,45,50,10]
[364,18,41,53,7]
[364.5,18.9,37,51,5]
[365,19,32,48,3]
[365.5,20,27,43,2.5]
[366,21.5,23,38,1.6]
[366.5,22,20,34,1.5]
[367,23,15,28,1.2]
[367.5,22,11,23,1]
[368,22.5,9,18,1.5]
[368.5,23.1,5,13,2.5]
[369,25.8,3,10,1.2]
[369.5,24.7,2.1,8,1.5]
[370,24.8,2.1,5,2.4]
[370.5,25.8,1.6,3.4,0.3]
[371,26,0.9,2.8,2.1]
[371.5,25.6,0.5,2,1.6]
[372,27.5,0.6,1.8,0.9]
[372.5,26.8,1.1,2.4,0.5]
[373,25.7,1.2,1.1,0.9]
[373.5,26.1,1.1,2.1,1.3]
[374,26,0.9,1.6,0.3]
[374.5,25,0.2,0.9,2.6]
[375,26.2,0.9,0.5,0.2]
[375.5,25.2,0.7,0.9,1.7]
[376,25.9,1.1,1.3,0.1]
[376.5,24,0.9,0.3,1.5]
[377,24.6,0.5,2.6,0.5]
[377.5,25.9,0.7,0.2,0.2]
[378,23.4,1.4,1.7,1.9]
[378.5,24.6,1.1,0.1,0.5]
[379,23.6,1,1.5,1.6]
[379.5,22.1,1.2,0.5,0.4]
[380,20.5,0.9,0.2,0.2]
[380.5,21.5,0.7,1.9,1.2]
[381,22.1,0.8,0.5,0.2]
[381.5,19.9,0.9,1.6,0.6]
[382,19,1.1,0.4,0.9]
[382.5,19,0.2,0.2,0.3]
[383,18.5,2.3,1.2,1.8]
[383.5,18.9,0.8,0.2,0.2]
[384,18,1.6,0.6,2.3]
[384.5,17.8,0.6,0.9,0.8]
[385,16.1,0.8,0.3,1.6]
[385.5,15.4,0.4,1.8,0.6]
[386,15.9,1,0.2,0.8]
[386.5,16.1,0.1,2.3,0.4]
[387,14.6,0.46,0.8,1]
[387.5,13.8,0.54,1.6,0.1]
[388,14.3,0.35,0.6,0.46]
[388.5,12.8,1.99,0.8,0.54]
[389,11.5,1.1,0.4,0.35]
[389.5,12.4,0.8,1,1.99]
[390,10.1,0.5,0.1,1.1]
[390.5,12,0.9,0.46,0.8]
[391,10.1,1.1,0.54,0.5]
[391.5,9.3,1.5,0.35,0.9]
[392,9.5,1.1,1.99,1.1]
[392.5,9,0.9,1.1,1.5]
[393,8.6,1.1,0.8,1.1]
[393.5,7.5,0.8,0.5,0.9]
[394,8.1,0.9,0.9,1.1]
[394.5,8.9,1.2,1.1,0.8]
[395,6.2,0.8,1.5,0.9]
[395.5,6.1,0.7,1.1,1.2]
[396,6.5,0.9,0.9,0.8]
[396.5,5.1,1.1,1.1,0.7]
[397,5.1,0.7,0.8,0.9]
[397.5,5.8,0.5,0.9,1.1]
[398,4.6,0.6,1.2,0.7]
[398.5,4.8,0.7,0.8,0.5]
[399,4.9,0.25,0.7,0.6]
[399.5,4.8,0.3,0.9,0.7]
[400,4.1,0.24,1.1,0.24]
[400.5,4.8,0.21,0.7,0.21]
[401,3.5,0.18,0.5,0.18]
[401.5,3.8,0.11,0.6,0.11]
[402,4,0.6,0.7,0.6]
[402.5,4.1,0.4,0,0.4]
[403,3.1,0.3,0.3,0.3]
[403.5,3.2,0.1,0.24,0.1]
[404,3.5,0.6,0.21,0.6]
[404.5,3.1,0.2,0.18,0.2]
[405,2.4,0.4,0.11,0.4]
[405.5,2.9,0.5,0.6,0.5]
[406,1.8,0.3,0.4,0.3]
[406.5,2.1,0.4,0.3,0.4]
[407,1.5,0.6,0.1,0.6]
[407.5,1.1,0.2,0.6,0.2]
[408,0.5,0.1,0.2,0.1]
[408.5,0.4,0.12,0.4,0.12]
[409,0.1,0.54,0.5,0.54]
[409.5,0.5,0.21,0.3,0.21]
[410,0,0,0.4,0]