{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"flags":["formulas_cached_only"]}
["Content","Disaggregation ","Specifications, type","Source","Year"]
["Landslide Events","Point","Binary","COE-M Quito","2005-2017"]
["Slope","50 m","Pre-normalized from continuous to weights (weighted classes) ","FUNEPSA et al., 2015",2015]
["Intense Precipitations (in 24 hours)","50 m","Pre-normalized from categorical to weights","FUNEPSA et al., 2015",2015]
["Soil Stability (from former landslides)","50 m","Pre-normalized from categorical to weights","FUNEPSA et al., 2015",2015]
["Lithology","50 m","Pre-normalized from categorical to weights ","FUNEPSA et al., 2015",2015]
["Land Use / Vegetation Cover","50 m","Pre-normalized from categorical to weights","FUNEPSA et al., 2015",2015]
["Seismicity","50 m","Pre-normalized from categorical to weights","FUNEPSA et al., 2015",2015]
["Population ","Block Scale","Continuous, normalized by natural breaks to weights","INEC",2010]
["Road Density","Street segment","Continuous, normalized by natural breaks to weights","STHV – MDMQ",2016]
["Total Built Area","Building Scale","Continuous, normalized by natural breaks to weights","STHV – MDMQ",2017]
["Building Footprint Area","Building Scale","Continuous, normalized by natural breaks to weights","STHV – MDMQ",2017]