	
	Microscope (*)
	RoboticScope©

	Working distance (cm)
	20-60 
	30-60 

	Magnification 
	1.0-17x
	2,7-30,1x

	Depth of field (cm)
	<1,2
	1,26

	Speed of movement 250 mm/s Immediate Immediate
	immediate
	250mm/sec

	Illumination
	Xenon, 300 W
	LED, 2-11W (extra-illumination from the HMD)

	Field of view (cm) 
	60
	5.8x4.3–64.5x48.4

	Learning curve 
	low
	low

	Stereopsis 
	yes
	yes

	Occupied space
	large
	large

	Image capture 
	2160 x 1080 pixel full‐HD LCD display/4K
	2 x 1600  x 1200 pixel/ merged 4K resolution (4928 x 2056 px) 

	Menu control 
	Manual, footplate
	Footplate and head movement

	Counterbalance system 
	Hydraulic
	Robotic

	Portability
	medium
	medium

	Teaching potential
	medium
	high

	Fluorescence
	yes
	N/A

	Weight (Kg)
	>225
	365





(*) data from LEICA, ZEISS microscope brochures (https://www.leica-microsystems.com/products/surgical-microscopes; www.zeiss.com/meditec/en/products/surgical-microscopes.html)
