Highlights
· Hydrophobic treatments significantly reduce moisture ingress in porous silicate materials.
· Optimized vacuum-based application enhances durability without altering porosity.
· Applications extend to contaminated soils, agriculture, permafrost, and infrastructures.
· Capillary absorption thresholds proposed as predictive durability indicators.
· Sustainable water management strategy aligning with environmental protection goals.
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