Highlights
· Hybrid model-free RL framework enhances real-time HVAC operational performance
· Real-building deployment achieves 17.27% reduction in HVAC energy use
· Method improves energy efficiency while maintaining acceptable thermal comfort
· Framework reduces manual intervention, lowering labor costs by 50 percent
· Scalable, model-free design enables rapid adoption across diverse building types
