· Chitosan can be used as an eco-friendly, cost-effective, biodegradable and non-toxic inhibitor for emerging green corrosion inhibition approaches.
· Multilayer inhibitor systems perform better corrosion inhibitory action for stainless steel Grade 202 (SS 202) through synergistic effect.
· [bookmark: _GoBack]Addition of TiO2 particles into chitosan or polyaniline coatings enhance the corrosion inhibition ability by adsorbing to pores thereby effectively covering the SS 202 metal surface.
· Multilayer inhibitor system (Polyaniline + Chitosan + TiO2) shows the smallest corrosion rate.

